

To Whom it May Concern,

Lott's Concrete precast and prestressed lintels have been designed and manufactured in accordance with the following standards:

Codes

Florida Building Code: FL17867-R2, FL17872-R2

Miami-Dade: Noa 18-0926.03

ASCE 7

ACI 318

ACI 530

Concrete

Precast Lintels: 4,000 psi

Prestressed Lintels: 6,000 psi

Grout per ASTM C476: 3,000 psi

Reinforcement

Rebar Placed in Lintel: ASTM A615 Gr 60

Rebar Placed in Field: ASTM A615 Gr 40 or 60

Prestressed Strand: ASTM A416 Gr 270

Masonry

Concrete Masonry Units: ASTM C90, 1,900 psi

Mortar: ASTM C270 Type M or S

Respectfully,

Rick Higgins GM. Lott’s Concrete Products Inc.